# [I-30364]  Stop charging when the cut-off SOC is reached

**Description:**

Use-Case Title: "Stop charging when the cut-off SOC is reached"

Goal: To notify and display the user that the charging stop SOC has been reached

Scope: SWP, Mobile App, Sound

Actors: driver, vehicle

Precondition:

1. [[~~I-25818~~] Start the charging process](#25818)

Trigger:

1. [the preset charging stop soc threshold is reached](#25810)
2. [charging stopped](#25804)

Requirement:

* The system notifies the driver that "charge cut-off SOC reached, charging completed" via out\_2, out\_5 and accompanied with soud out\_25
* The final SOC value display on out\_2, and out\_5