# [I-30365]  Start the Charging Process via Soft Switch

**Description:**

Use-Case Title: "Start the Charging Process via Soft Switch"

Goal: the driver can navigate to the charging switch to start the charging

Scope: SWP, Mobile App

Actors: driver/user, vehicle

Preconditions:

1. The vehicle is in Parking mode.
2. The charging cable is plugged in.

Trigger：

1. The user initiates the start of the charging process via the soft switch on out\_2. SWP and out\_5.Mobile App.

Main Scenario:

1. The user navigates to the charging interface on the out\_2. SWP or out\_5. Mobile App.
2. The user presses the "Start Charging" soft switch button.
3. The system checks if the vehicle is in Parking mode and the charging cable is plugged in.
4. The system sends a command to start the charging process.
5. The system displays a notification via out\_2. SWP or out\_5. Mobile App that the charging session has been successfully started.
6. [The charging process is in progress.](#25808)