Mute or pause function

**Functional Description**

When playing online radio stations, pause operation can be performed, and live programs can be muted. It can only be used when the vehicle is stopped through SWP operation.

Enabling conditions (a & b);

IVI system startup;

User operable display screen.

Trigger conditions (a | b | c):

When a valid network radio station is running, click the mute / pause soft button.

When a valid network radio station is running, mute / pause is controlled by the Switches hard button (Switches\_L\_Accept\_Cmd (vehicle / cabin / steering-wheel / left-area / accept / command) = 0x1: Press).

When an effective network radio station is running, use the Switches hard keys to control mute/pause (Switches\_L\_Accept\_Cmd (vehicle/cabin/steering-wheel/left-area/accept/command) = 0x1: Press).

When an effective network radio station is running, mute/pause is controlled through voice function.

Execution output (a&b&c):

When the network radio is playing, click the mute/pause soft button or use the Switches hard keys or voice control to mute or pause the network radio.

When the network radio is muted, the system shuts down, and the radio automatically plays sound the next time it is powered on.

Exit conditions (a|b)

System shutdown;

IVI system shutdown;

Switch audio source.

The SWP network radio page provides mute/pause soft buttons.

The Switches provide a mute/pause hard keys.

The voice recognition system can recognize mute/pause voice commands.

The SWP network radio page provides mute/pause soft buttons.

The Switches provide a mute/pause hard keys.

The voice recognition system can recognize mute/pause voice commands.